0/1 = absolute refuse/accept

User Interface Control Module

• Gather simulation runtime parameters input, including RCS target, incident angle of transmitter radar, display resolution and other parameters related to simulation and graphics display

Scheduling Module 1 for CM5

Scheduling Module 2 for iPSC/860

Scheduling Module 3 for IBM SP2

Scheduling Module 4 for Alpha Farm

Scheduling Module x for others

(simulation-related scheduling parameters)

(extensible to others)

Filter Module

• Choose one or more of the platforms based on the scheduling factors received

Simulation Module 1 for CM5

Simulaton Module 2 for iPSC/860

Simulation Module 3 for IBM SP2

Simulation Module 4 for Alpha Farm

Simulation Module x for others

(extensible to others)

(Decision Vector)

Mapper Module

• Μap numerical results to (AVS) graphical format

(AVS) Geometry Viewer Module

• Graphic display of simulation output

scheduling factor: 0 - 1