user runtime input

IBM RS/6000 (local machine)

Fig. 6 System configuration of the prototype integration system

SUN Spar c 2 (remote)

SUN Spar c 1+ (remote)

. control processor(CP) of the CM5 . running the module ‘Partial donor-cell’

32-node Connection Machine 5

. running the CMFortran module ‘van Leer’

. running AVS kernel and the module ‘graph viewer’ . displaying system control panel and the GUI windows

. running the module ‘Advection Interface’

Local area network

. running the module

‘Lax-Wendroff’

DEC5000 (remote)

. running the module

‘Hain’ . running ”AVS/CM interface part” of the CMFortran module ‘van Leer’

. running CMMD host program of the

module ‘Donor-cell’

. running CMMD node program of the module

‘Donor-cell’