CREATING REGULAR SENDING PORTS

Figure 4

Parent

Child A

Child B

B) By Passing a Port in a Message

1) Parent sends the Port P1 through the Channel Channel2

2) Child B receives this Port, which is installed as P3

3) The P3 Port points at the Child A’s Standard Receiving Port

Channel0

Channel1

P1 P2

P2