19XR 6-Page Brochure  							 
Revised New Copy
Cat. #819-126
Sage #320-1091

INSIDE COVER:

Background Photo:  “Rain Forest” wallpaper

Head:
Carrier’s Evergreen Chillers: The Chlorine-Free Way to World-Class Efficiency -- Without Compromise.

Copy:
Introducing a significant breakthrough in chiller technology. The Evergreen Chillers from Carrier.

For the first time ever, you don’t have to choose between high efficiency and environmental responsibility, or between operating savings and long-term protection from refrigerant phaseout. With Evergreen, you can have it all.

Sub:
Highest Efficiency

Copy:
Using advanced aerodynamic design principles, Carrier engineers have optimized Evergreen Chillers to deliver efficiency levels of .52 kW/ton or better at standard ARI conditions with chlorine-free HFC-134a. No other manufacturer can make that claim.

Sub:
Environmentally Responsible

Copy:
Evergreen Chillers don’t compromise on environmental responsibility either -- they use safe, HFC-134a, a non-ozone depleting refrigerant. That also means you don’t have to worry about costly machine conversions as chlorine-based refrigerants, such as HCFCs, are phased out in the near future.

Plus, the Evergreen Chiller’s high energy efficiency minimizes the amount of electricity needed. Ultimately, that means burning less fossil fuel, a prime source of greenhouse gases.

Sub:
Best Overall Value

Copy:
Evergreen Chillers won’t compromise your wallet, either. All in all, you’ll get the best efficiency and the best refrigerant at competitive prices. No compromise about it.

INSIDE SPREAD (call-outs)

Copy:
Advanced turbine technology allows the Evergreen Chiller to achieve rebate-qualifying energy consumption levels of .52 kW/ton or better. This optional feature make Evergreen the most efficient chlorine-free chiller in the world.

Copy:
Compact design allows for open-top container shipment on overseas installations, maintaining “factory-fresh” conditions, while reducing the cost of transportation.

Copy:
Carrier’s hermetic motors are liquid-refrigerant cooled. Designed for superior reliability, hermetic motors eliminate shaft seal leakage and wear, as well as additional machine room cooling requirements characteristic of open-drive, air-cooled motors.

Copy:
Isolation valves, available on all Evergreen chillers, allow the refrigerant to be stored inside the chiller during servicing, eliminating the need for bulky refrigerant storage tanks.

Copy:
Bolt-together construction ensures ease of disassembly and reassembly at the job site, reducing installation time and expense while maintaining product quality and design integrity. Video instructions take you through the process, step by step.

Copy:
User-friendly Product Integrated Control (PIC) digitally monitors over 100 functions and displays over 125 operating and diagnostic conditions from allowing simple monitoring of day-to-day operations. 

Copy:
HFC-134a refrigerant has zero ozone-depletion potential and is classified as an A1 refrigerant by ASHRAE, the safest category possible. And with the production of  HFC-134a on the rise, you’ll always have a readily available supply of safe refrigerant at reasonable prices for the life of your Evergreen chiller.

BACK GATE

Sub:
Engineered for Efficiency

Copy:
Now, the best value in chillers delivers world-class efficiency, chlorine-free.

Carrier engineers have enhanced existing compressor technology to achieve efficiencies once available only in chillers using chlorine-based refrigerants. The Evergreen’s centrifugal compressor is built around an advanced impeller and tunnel diffuser, redesigned for optimal efficiency using HFC-134a. 

With the addition of Carrier’s patented turbine technology, efficiencies of .52 kW/ton and better are possible. The turbine recovers energy typically wasted in the conventional expansion portion of the vapor compressor cycle. Connected to the motor rotor, the turbine lightens the motor’s workload and reduces the chiller’s external power requirements.

For added efficiency, Evergreen Chillers are available with a range of heat exchanger frame sizes to optimize your chiller for your specific application.

Subhead:
Sized to Fit

Copy:
To run on chlorine-free HFC-134a refrigerant, the Evergreen Chiller uses a positive-pressure design.
Positive-pressure chillers are typically 35% smaller than negative-pressure machines of comparable capacities. That means you’ll need less mechanical room floor space -- and the Evergreen Chiller’s take-apart construction makes getting it there a lot easier. 

With positive-pressure design, no purge is required, and there’s no need for expensive refrigerant containment add-ons -- optional built-in isolation valves allow you to store refrigerant inside the chiller during servicing.

Sub:
Reliable Design -- Backed by 25 Years’ Experience

Copy:
The Evergreen Chiller’s reliability begins with the compressor. Twenty-five years of successful operating experience go into each hermetic compressor motor. Because they’re refrigerant cooled, hermetic motors run cooler and cleaner, and last longer. 

The Evergreen’s single-stage compressor is design around a stationary tunnel diffuser to optimize chiller efficiency while keeping the total number of moving parts to a minimum. With the addition of a single moving part -- the high-efficiency turbine -- the Evergreen chiller achieves efficiencies of .52 kW/ton or better.

ASME-certified heat exchangers further contribute to the Evergreen Chiller’s reliability. They’re built to withstand four times normal operating pressure, ensuring leak-tight integrity.

Another high-reliability feature is the Accumeter refrigerant flow control meter, which increases part-load efficiency and optimizes chilled water capacity -- all with just a single moving part.

Sub: 
Easy to Use

Copy:
The Evergreen Chiller is designed for direct digital control using Carrier’s Product Integrated Control (PIC) system. Operator-friendly and easy-to-use, PIC monitors over 100 functions and displays over 125 operating and diagnostic conditions. The Evergreen’s controls are completely compatible with Carrier’s Comfort Network (CCN to let you monitor and control all HVAC functions from one location using a personal computer.

BACK PAGE 

Head:
A Tradition of Environmental Leadership

Copy:
The Carrier Corporation continues to receive recognition for its environmental leadership.  Carrier is a 1995 recipient of the coveted National Energy Award, presented by the U.S. Department of Energy for energy-related programs that benefit the nation’s environment, economy and security.  Carrier also has won the EPA’s Stratospheric Ozone Protection Award for advanced technology designed to improve the operating efficiency of HFC-134a centrifugal chillers.  We’re equally proud of our New York State Governor’s Awards...for Environmental Excellence and Innovation in Energy.

Sub: 
A Full Range of  Services

Copy: 
Carrier is committed to helping you keep your new Evergreen Chiller running at peak efficiency. A full range of  service options are available, from our comprehensive Total Retrofit Solutions (TRS) program to service agreements tailored to your specific needs. Extended warranty and financial agreements are also available.

Sub:
The One Choice With No Compromises...

Copy: 
If you’re contemplating a new chiller purchase, there’s only one choice with no compromises -- the new Evergreen Chiller.  To find out more about how Carrier can help you save on operating costs today, while protecting your investment for the future, contact your local Carrier representative. Or call 1-800-CARRIER.

Caption (for award graphic):
The National Energy Award, presented by the Department of Energy, reflects Carrier’s commitment to fostering programs that promote energy conservation, responsible energy use and environmental health.

[Bob--Also needed are the following approvals:  ARI, UL, ASME and CSA. Let me know which, if any of these you need. Thanks.]